|  |  |  |
| --- | --- | --- |
| **Company Name:**Site: |  | COSHH Assessment |
|  |  |  |  |  |
| Supplier: | CHAUCER SOLUTIONS LTD | COSHH Number | 08 |
|  |  | page 1 |
| Assessment By: | Activity: | Review Date | Assessment Date |
|  | Cleaning and lubrication of scaffolding clips |  |  |
|  | Persons/Groups at Risk |  |  |
|  | Scaffolders |  |  |

|  |
| --- |
| **NAME OF HAZARDOUS SUBSTANCE USED OR CREATED** |
| **Substance: Clip Free** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Flammable |  | Oxidising |  |  |  | http://www.hse.gov.uk/chemical-classification/images/pictogram-gallery/irritant.gif |  | Health hazard |  | Corrosive |
| **FLAMMABLE** |  | **OXIDISING** |  | **EXPLOSIVE** |  | **IRRITANT** |  | **HARMFUL** |  | **CORROSIVE** |
| **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | NO |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Insert ✓ in appropriate boxes |
|  |  | Toxic |  |  |  |  |  |  |  |  |
| **COMPRESSED GAS** |  | **TOXIC** |  | **HARMFUL TO THE EINVIRONMENT** |  |  |  |  |  |  |
| **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | NO |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Insert ✓ in appropriate boxes |

|  |  |  |  |
| --- | --- | --- | --- |
| Please add comments into boxes where required. | Insert ✓ in appropriate boxes | **YES** | **NO** |
| Is Manufacturers Safety Data Sheet available? |  | ✓ |  |
| Does the Substance have a Workplace Exposure Limit (WEL)?  |   | ✓ |  |
| If the substance has a WEL please state. if un-sure check HSE document – EH40 | 5mg/m3 | ✓ |  |
| Can a safer substance be used or can the substance be enclosed or extracted. |  |  | ✓ |
| Will employees be given information and training? |  |  | ✓ |
| Will Personal Protective Equipment be provided for employees? |  |
|  State the standard of RPE (respirators) | Not necessary in well ventilated areas |  | ✓ |
|  State the standard of Goggles or Spectacles | BS EN166 safety glasses | ✓ |  |
|  State the standard of Gloves | Nitrile/PVC gloves to be worn | ✓ |  |
|  State the standard of Overalls |  |  | ✓ |
|  State the standard of Boots | BS EN345 | ✓ |  |
|  Other Equipment | Attach details if YES |  | ✓ |
| Will Exposure Monitoring and/or Control Measures be required? | Attach details if YES |  | ✓ |
| Will Health Surveillance be necessary? | Attach details if YES |  | ✓ |
| Does this Substance need to be disposed of by a Waste Disposal Contractor? | ✓ |  |
| Have all necessary First-aid requirements been provided? |  | ✓ |  |
| Have Storage requirements for the substance been provided/arranged on site? |  | ✓ |  |
| **FIRST AID, FIRE FIGHTING, STORAGE & HANDLING, DISPOSAL AND ACCIDENTAL RELEASE INSTRUCTIONS ARE PROVIDED ON PAGES 2 & 3** | **Number of Sheets attached to this Assessment** |  |
| FIRST AID INSTRUCTIONS |
| **Route of Exposure, or****Type of Injury** | **First Aid Treatment** |
| Skin Contact  | Wash skin with large amounts of water. If irritation persists seek medical advice |
| Eye Contact  | Irrigate with eyewash solution or clean water, holding eyelids apart for 10 minutes.Get immediate medical attention. |
| Inhalation  | Remove from exposure, rest and keep warm. Seek immediate medical attention. |
| Ingestion | Wash out mouth with water. Do not induce vomiting. Give water to drink if patient feelsunwell. Get medical attention immediately. |
| General Information |  |

|  |
| --- |
| **FIRE FIGHTING MEASURES** |
| **Hazard** | **Measures** |
| Fire  | Extinguish with Dry Powder, Foam or Water Fog. Do not use water jets.Fires in closed or confined spaces should be tackled by trained personnel who should wear breathing apparatus. Possible risk of can rupture when exposed to fire/high temperatures. |
| Stability | Stable under normal temperature conditions. May react with strong oxidising materials. |
| Decomposition Products | Fire or high temperatures create halogenated hydrocarbons oxides of carbon. |

|  |
| --- |
| **MANUFACTURERS INFORMATION** |
| **Manufacturers Name and Address** | CHAUCER SOLUTIONS LTDLEYCOURT FARMGT GRANSDENBEDSSG19 3AS |
| **Manufacturers Health & Safety Data Sheet Reference** | N/A |
| **24 Hour Emergency Telephone Number** | 01767 677445 |
| **Regulatory Information: Warning Label Phrases** | Not classified as hazardous for supply. No statutory label required. |

|  |  |
| --- | --- |
| **Regulatory Information: Warning Label Phrases** | Not regarded as a health or environmental hazard under current legislation. |

|  |
| --- |
| **STORAGE AND HANDLING** |
| **Hazard** | **Measures** |
| Handling  | Avoid spilling, skin and eye contact. |
| Storage | Store upright in container provided. Avoid extremes of temperature. |

|  |
| --- |
| DISPOSAL MEASURES |
| **Hazard** | Measures |
| Pollution of water courses or drains | Small spillages: Rinse with water into the drain. Large spillages: Absorb with granules. |

|  |
| --- |
| ACCIDENTAL RELEASE MEASURES |
| **Hazard** | Measures |
| Spillage | Small spillages: Rinse with water into the drain. Large spillages: Absorb with granules. |

|  |
| --- |
| USAGE/EXPOSURE |
| **Frequency and Duration of use** |  |
| **Maximum number of people involved in activity** |  |
| **Quantities stored/used** |  |
| **Exposure levels** |  |

**Safe System of Work**

1. Wash at the end of each work shift and before eating, smoking and using the toilet.

2. Ensure spill kit is close at hand.

3. Ensure PVC/Nitrile gloves are worn.

4.

5.

6.

7.

8.

**Operatives Acknowledgement**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name:** | **Signature:** | **Date:** | **Name:** | **Signature:** | **Date:** |
|  |   |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |