|  |  |  |
| --- | --- | --- |
| **Company Name:**Site: |  | **COSHH** **Assessment** |
|  |  |  |  |  |
| Supplier: | British Gypsum | COSHH Number | 34 |
|  |  | page 1 |
| Assessment By: | Activity: | Review Date | Assessment Date |
|  | Sealing Substrate |  |  |
|  | Persons/Groups at Risk |  |  |
|  | User and others in immediate vicinity. |  |  |

|  |
| --- |
| **NAME OF HAZARDOUS SUBSTANCE USED OR CREATED** |
| **Substance: Thistle Bond IT** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |
| **FLAMMABLE** |  | **OXIDISING** |  | **EXPLOSIVE** |  | **IRRITANT** |  | **HARMFUL** |  | **CORROSIVE** |
| **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | NO |
|  |  |  |  |  |  |  |  |  | ✓ |  |  |  |  |  |  |  |
| Insert ✓ in appropriate boxes |
|  |  |  |  |  |  |  |  |  |  |  |
| **COMPRESSED GAS** |  | **TOXIC** |  | **HARMFUL TO THE EINVIRONMENT** |  |  |  |  |  |  |
| **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | **NO** |  | **YES** | NO |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Insert ✓ in appropriate boxes |

|  |  |  |  |
| --- | --- | --- | --- |
| Please add comments into boxes where required. | Insert ✓ in appropriate boxes and add comment below | **YES** | **NO** |
| Is Manufacturers Safety Data Sheet available? |  | ✓ |  |
| Does the Substance have a Workplace Exposure Limit (WEL)?  |   |  | ✓ |
| If the substance has a WEL please state. if un-sure check HSE document – EH40 | **N/A** |  |  |
| Can a safer substance be used or can the substance be enclosed or extracted. |  | ✓ |  |
| Will employees be given information and training? |  | ✓ |  |
| Will Personal Protective Equipment be provided for employees? |  |
|  State the standard of RPE (respirators) | Required where risk assessment indicates refer to SDS for further info |  |  |
|  State the standard of Goggles or Spectacles | Required where risk assessment indicates | ✓ |  |
|  State the standard of Gloves | Required where risk assessment indicates | ✓ |  |
|  State the standard of Overalls |  |  |  |
|  State the standard of Boots |  | ✓ |  |
|  Other Equipment | Attach details if YES |  |  |
| Will Exposure Monitoring and/or Control Measures be required? | Attach details if YES |  | ✓ |
| Will Health Surveillance be necessary? | Attach details if YES |  | ✓ |
| Does this Substance need to be disposed of by a Waste Disposal Contractor? |  |  |
| Have all necessary First-aid and welfare requirements been provided? |  | ✓ |  |
| Have Storage requirements for the substance been provided / arranged on site? |  | ✓ |  |
| **FIRST AID, FIRE FIGHTING, STORAGE & HANDLING, DISPOSAL AND ACCIDENTAL RELEASE INSTRUCTIONS ARE PROVIDED ON PAGES 2 & 3** | **Number of Sheets attached to this Assessment** |  |
| FIRST AID INSTRUCTIONS |
| **Route of Exposure, or****Type of Injury** | **First Aid Treatment** |
| Skin Contact  |  It is important to remove the substance from the skin immediately. In the event of any sensitisation symptoms developing, ensure further exposure is avoided. Remove contamination with soap and water or recognised skin cleansing agent. Get medical attention if symptoms are severe or persist after washing. |
| Eye Contact  | In case of contact with eyes, rinse immediately with plenty of water for at least 10 minutes with the eyelids open and seek medical advice. |
| Inhalation  | Remove affected person from source of contamination. Move affected person to fresh air and keep warm and at rest in a position comfortable for breathing. Maintain an open airway. Loosen tight clothing such as collar, tie or belt. When breathing is difficult, properly trained personnel may assist affected person by administering oxygen. Place unconscious person on their side in the recovery position and ensure breathing can take place. |
| Ingestion | Rinse mouth thoroughly with water. Give a few small glasses of water or milk to drink. Stop if the affected person feels sick as vomiting may be dangerous. Do not induce vomiting unless under the direction of medical personnel. If vomiting occurs, the head should be kept low so that vomit does not enter the lungs. Never give anything by mouth to an unconscious person. Move affected person to fresh air and keep warm and at rest in a position comfortable for breathing. Place unconscious person on their side in the recovery position and ensure breathing can take place. Maintain an open airway. Loosen tight clothing such as collar, tie or belt. |
| General Information | Get medical attention immediately. Show this Safety Data Sheet to the medical personnel |

|  |
| --- |
| **FIRE FIGHTING MEASURES** |
| **Hazard** | **Measures** |
| Fire  | Extinguish with alcohol-resistant foam, carbon dioxide, dry powder or water fog. Use fire extinguishing media suitable for the surrounding fire. |
| Stability | Avoid temperatures over 30°C and below 5°C. Avoid contact with acids. |
| Decomposition Products | Product is not known to cause long-term environmental effects, if disposed of correctly. Product should not be allowed to enter drains/watercourses or allowed to reach ground/surface water. |

|  |
| --- |
| **MANUFACTURERS INFORMATION** |
| **Manufacturers Name and Address** | British GypsumEast LeakeLoughboroughLeicestershireLE12 6HX |
| **Manufacturers Health & Safety Data Sheet Reference** |  |
| **24 Hour Emergency Telephone Number** | 0844 800 1991bgtechnical.enquiries@bpb.com |
| **Regulatory Information: Warning Label Phrases** | H317 May cause an allergic skin reactionP102 Keep out of reach of children. P261 Avoid breathing dust or mist. P280 Wear protective gloves/ protective clothing/ eye protection/ face protection. P302+P352 IF ON SKIN: Wash with plenty of water. P333+P313 If skin irritation or rash occurs: Get medical advice/ attention. P501 Dispose of contents/ container in accordance with national regulations  |

|  |
| --- |
| **STORAGE AND HANDLING** |
| **Hazard** | **Measures** |
| Handling  | This product is not classed as hazardous for the purposes of transportation. |
| Storage | Buckets should be stacked in a safe and stable manner. Store in dry conditions between 5 and 30°C. Protect from frost and direct sunlight.  |

|  |
| --- |
| DISPOSAL MEASURES |
| **Hazard** | Measures |
| Pollution of water courses or drains | Should be disposed of at a suitable landfill site in accordance with local environmental regulations.  |

|  |
| --- |
| ACCIDENTAL RELEASE MEASURES |
| **Hazard** | Measures |
| Spillage | Product is not known to cause long-term environmental effects, if disposed of correctly. Product should not be allowed to enter drains/watercourses or allowed to reach ground/surface water. |

|  |
| --- |
| USAGE/EXPOSURE |
| **Frequency and Duration of use** | N/A |
| **Maximum number of people involved in activity** | N/A |
| **Quantities stored/used** | N/A |
| **Exposure levels** | N/A |

**Safe System of Work**

1.

2.

3.

4.

5.

6.

7.

8.

9.

10.

**Operatives Acknowledgement**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name:** | **Signature:** | **Date:** | **Name:** | **Signature:** | **Date:** |
|  |   |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |